**Models: ADJ-B BACnet WALL ADJUSTER (Remote set point adjustment)**

GUIDE SPECIFICATION

(Suitable for the CSI Master Format)

BACnet™ protocol VAV diffusers shall be supplied with a remote set point adjuster model ADJ-B manufactured by Acutherm, Hayward CA.

The set point adjuster shall be a remote sensor for the diffuser and not require a separate BACnet connection and shall have a simple plug connection to the diffuser with no required set up for communication or operation.

The adjuster shall provide occupant set point adjustment and optional room temperature measurement. The room temperature sensor shall be factory calibrated, but allow for re-calibration if required.

The set point adjuster shall allow adjustment of room temperature set point in F or C and numerical or warmer/cooler bars.

Optionally the adjuster shall also provide configuration of any secondary M-Series (motorized) diffuser’s minimum and maximum damper positions.